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1. Introduction
This Heritage Statement supports an application for Listed Building Consent for essential external repair works to a Grade II Listed Building. These works are required to address deterioration,  prevent water ingress, and preserve the historic fabric using conservation-led, like-for-like repair methods. As well as addressing health & Safety concerns.

The evaluation is prepared in accordance with:
• Planning (Listed Buildings and Conservation Areas) Act 1990
• NPPF (2023) sections relating to conserving heritage assets
• Historic England guidance on masonry, mortars, brick replacement and repair

The works are designed to ensure minimal intervention, maximum retention of original fabric, and long-term protection of the building.

2. Significance of the Listed Building
The building’s significance derives from its:

Architectural Value
• Historic brick façade with traditional bonding and joint profiles
• Characteristic detailing, rainwater goods, and construction methods

Historic Value
• Contribution to the historic townscape
• Representation of local craftsmanship and vernacular materials

Townscape Value
• Strong visual contribution to the character of its street and surrounding context

3. Description of Proposed Works
3.1 Scaffolding
Temporary and fully reversible scaffolding will be erected to allow safe access for repairs.

3.2 Removal of Failed Render
Areas of cracked, blown or delaminated render will be carefully removed by hand to expose original brickwork.

3.3 Brickwork Repairs
Damaged or spalled bricks will be repaired or replaced where necessary using a conservation-led brick matching strategy.

3.4 Pointing & Jointing Repairs
Mortar joints will be raked by hand and repointed using a breathable lime mortar matched to the original mix, colour and profile.

3.5 Gutter Repairs
Gutters will be repaired on a like-for-like basis, retaining traditional profiles and materials.

3.6 Lead Flashing & Brick Slip Installation
Lead flashing will be installed in accordance with conservation standards, and brick slips will reinstate lost finishes in areas previously rendered.

4. Brick Matching Strategy
4.1 Visual and Dimensional Matching
Replacement bricks will be matched to the existing historic brickwork in:
• Colour (including natural variations and weathering tone)
• Texture (to replicate original surface finish)
• Size and dimension (imperial dimensions where required)
• Bond pattern (ensuring continuity with historic bonding)

4.2 Material Compatibility
Bricks will be:
• Clay-fired in a similar manner to the original
• Of a similar porosity and density to avoid incompatibility
• Frost-resistant and suitable for external heritage use

4.3 Sourcing Strategy
Bricks may be sourced from:
• Specialist heritage brick manufacturers
• Salvaged bricks from matching period stock
• Reclaimed bricks from conservation suppliers

4.4 Sample Panel Approval
A sample repair panel will be prepared onsite to confirm brick match quality, mortar colour, and joint finish. This will be provided for approval by the Conservation Officer.

4.5 Installation
Bricks will be installed using lime mortar compatible with the existing fabric. No cement-based mortars will be used.

5. Impact Assessment
5.1 Architectural Significance
The works sustain the building’s architectural character through appropriate brick matching, reinstatement of traditional joint profiles, and sensitive use of materials.

5.2 Historic Fabric
The approach avoids unnecessary replacement and ensures maximum retention of original materials.

5.3 Setting
As the works are repair-based and visually sympathetic, there is no negative impact on the building’s setting.

6. Policy Compliance
The proposal complies with:
NPPF (2023)
• Paragraph 199: Conservation appropriate to significance
• Paragraphs 200–202: No harm; repairs preserve existing character

Planning (Listed Buildings and Conservation Areas) Act 1990:
• Section 16: Special regard given to the preservation of the asset
• Section 66: No harm to special architectural or historic interest

Historic England Guidance:
• Mortars, Renders & Plasters
• Practical Building Conservation – Masonry
• Principles of Repair

7. Conclusion
The proposed works are essential conservation repairs that will safeguard the building’s long-term condition, preserve and enhance historic brickwork, and use materials and methods in line with best conservation practice.

The works cause no harm to the listed building’s special architectural or historic interest and are fully appropriate for Listed Building Consent.

